000     @SCRATCH
001     @SCRATCH
001     _RETURN_
002     @SCRATCH
003     @SCRATCH
004-005 strtok.save
006-007 DL_Offset
008-009 cmdOffset
00A-00B cmdBufferRd
00C-00D cmdBufferWr
00E     ft800Gpio
00F     num_cha
010-011 intA
012-013 intB
014-015 intC
016-017 intD
018-019 intE
01A-01B intF
01C-01D fracA
01E-01F fracB
020-021 fracC
022-023 fracD
024-025 fracE
026-027 fracF
028-029 sig_A
02A-02F int_A
030-035 frac_A
036-037 sig_B
038-03D int_B
03E-043 frac_B
044-045 sig_C
046-04B int_C
04C-051 frac_C
052-053 sig_D
054-059 int_D
05A-05F frac_D
060-061 sig_E
062-067 int_E
068-06D frac_E
06E-06F sig_F
070-075 int_F
076-07B frac_F
07C-07D @sprintf_string
07E-081 FT800memRead8.addr
07E-081 User_App.def
07E     FT800_HostCmdWrite.Command
07E     @delay_ms1.P1
07E-0AF Touch_Calibrate.strbuf
07E-081 FT800memWrite8.addr
07E     FT800_Initial.@SCRATCH1
07F     FT800_Initial.@SCRATCH2
080     FT800_Initial.@SCRATCH3
081     FT800_Initial.@SCRATCH4
082     FT800memRead8.data8
082     User_App.sig
082     FT800memWrite8.data8
083-084 @DIV1616.P1
083-084 Update_Screen.sigA
083-086 FT800memRead32.addr
083     FT800memWrite8.@SCRATCH1
083     FT800memRead8.@SCRATCH1
083     Conv_hex_to_Ascii.@SCRATCH1
083     User_App.@SCRATCH1
084     FT800memWrite8.@SCRATCH2
084     FT800memRead8.@SCRATCH2
084     Conv_hex_to_Ascii.@SCRATCH2
084     User_App.@SCRATCH2
085-086 Update_Screen.sigB
085-086 @DIV1616.P1
085     FT800memWrite8.@SCRATCH3
085     FT800memRead8.@SCRATCH3
085     User_App.@SCRATCH3
086     FT800memWrite8.@SCRATCH4
086     FT800memRead8.@SCRATCH4
086     User_App.@SCRATCH4
087-088 Update_Screen.sigC
087-08A FT800memRead32.data32
087     FT800memWrite8.@SCRATCH5
087     FT800memRead8.@SCRATCH5
087     @DIV1616.@SCRATCH1
087     User_App.@SCRATCH5
089-08A Update_Screen.sigD
08B-08E FT800memRead32.dat
08B-08C Update_Screen.sigE
08D-08E Update_Screen.sigF
08F-090 Update_Screen.valA
08F     FT800memRead32.@SCRATCH1
090     FT800memRead32.@SCRATCH2
091-092 Update_Screen.valB
091     FT800memRead32.@SCRATCH3
092     FT800memRead32.@SCRATCH4
093-094 Update_Screen.valC
093     FT800memRead32.@SCRATCH5
095-096 Update_Screen.valD
097-098 Update_Screen.valE
099-09A Update_Screen.valF
09B-09C Update_Screen.facA
09D-09E Update_Screen.facB
09F-0A0 Update_Screen.facC
0A1-0A2 Update_Screen.facD
0A3-0A4 Update_Screen.facE
0A5-0A6 Update_Screen.facF
0A7-0D8 Update_Screen.strbuf
0B0     Touch_Calibrate.@SCRATCH1
0B1     Touch_Calibrate.@SCRATCH2
0B2     Touch_Calibrate.@SCRATCH3
0B3     Touch_Calibrate.@SCRATCH4
0D9-0DA Text_CMD.str
0D9-0DC Start_CMDList.screen_color
0D9     @PSTRINGC_292.@SCRATCH1
0D9     End_CMDList.@SCRATCH1
0DA     @PSTRINGC_292.@SCRATCH2
0DA     End_CMDList.@SCRATCH2
0DB-0DC Text_CMD.x
0DB     @PSTRINGC_292.@SCRATCH3
0DB     End_CMDList.@SCRATCH3
0DC     @SPRINTF.P1
0DC     End_CMDList.@SCRATCH4
0DD-0DE Text_CMD.y
0DD-0E0 FT800memRead16.addr
0DD     Start_CMDList.@SCRATCH1
0DE     Start_CMDList.@SCRATCH2
0DF-0E0 Text_CMD.font
0DF     Start_CMDList.@SCRATCH3
0E0     Start_CMDList.@SCRATCH4
0E1-0E2 Text_CMD.opt
0E1-0E2 FT800memRead16.data16
0E1     Start_CMDList.@SCRATCH5
0E2     Start_CMDList.@SCRATCH6
0E3-0E4 FT800memRead16.dat
0E3-0E6 Text_CMD.tx_color
0E3     Start_CMDList.@SCRATCH7
0E4     Start_CMDList.@SCRATCH8
0E5     FT800memRead16.@SCRATCH1
0E6     FT800memRead16.@SCRATCH2
0E7-0E8 End_incCMDOffset.currentOffset
0E7-0E8 incCMDOffset.currentOffset
0E7     FT800memRead16.@SCRATCH3
0E7     Text_CMD.@SCRATCH1
0E8     FT800memRead16.@SCRATCH4
0E8     Text_CMD.@SCRATCH2
0E9     End_incCMDOffset.commandSize
0E9     incCMDOffset.commandSize
0E9     FT800memRead16.@SCRATCH5
0E9     Text_CMD.@SCRATCH3
0EA-0EB End_incCMDOffset.newOffset
0EA-0EB incCMDOffset.newOffset
0EA     Text_CMD.@SCRATCH4
0EB-0EE FT800memWriteStr.addr
0EB-0EE FT800memWrite16.addr
0EB     Text_CMD.@SCRATCH5
0EC     End_incCMDOffset.@SCRATCH1
0EC     Text_CMD.@SCRATCH6
0ED     End_incCMDOffset.@SCRATCH2
0ED     Text_CMD.@SCRATCH7
0EE     Text_CMD.@SCRATCH8
0EF-0F2 FT800memWrite32.addr
0EF-0F0 FT800memWriteStr.str
0EF-0F0 FT800memWrite16.data16
0F1-0F2 FT800memWriteStr.i
0F1     FT800memWrite16.@SCRATCH1
0F2     FT800memWrite16.@SCRATCH2
0F3-0F6 FT800memWrite32.data32
0F3     FT800memWrite16.@SCRATCH3
0F3     FT800memWriteStr.@SCRATCH1
0F4     FT800memWrite16.@SCRATCH4
0F4     FT800memWriteStr.@SCRATCH2
0F5     FT800memWrite16.@SCRATCH5
0F5     FT800memWriteStr.@SCRATCH3
0F6     FT800memWriteStr.@SCRATCH4
0F7     FT800memWrite32.@SCRATCH1
0F7     FT800memWriteStr.@SCRATCH5
0F8     FT800memWrite32.@SCRATCH2
0F9     FT800memWrite32.@SCRATCH3
0FA     FT800memWrite32.@SCRATCH4
0FB     FT800memWrite32.@SCRATCH5
0FC     spi_rw.Db
0FD     spi_rw.bt
0FE     spi_rw.result
0FF     spi_rw.@SCRATCH1
F71     CCP_5_LOW
F71     CCP_5
F72     CCP_5_HIGH
F74     CCP_4
F74     CCP_4_LOW
F75     CCP_4_HIGH
F83     PSP_DATA
FB4.6   C1OUT
FB4.7   C2OUT
FB8     CCP_3_LOW
FB8     CCP_3
FB9     CCP_3_HIGH
FBB     CCP_2
FBB     CCP_2_LOW
FBC     CCP_2_HIGH
FBE     CCP_1_LOW
FBE     CCP_1
FBF     CCP_1_HIGH
FE1-FE2 @READ_PACKED_MEMORY.P1
FE1-FE2 @WRITE_PACKED_MEMORY.P2
FE9-FEA @READ_PROGRAM_MEMORY.P1
FE9-FEA @WRITE_PACKED_MEMORY.P2
FE9-FEA @READ_PACKED_MEMORY.P3
FE9-FEA @WRITE_PROGRAM_MEMORY.P4
FF6-FF8 @WRITE_PROGRAM_MEMORY.P1
FF6-FF8 @READ_PROGRAM_MEMORY.P2

ROM Allocation:
000146  @delay_ms1
001F70  MAIN
000134  init_port
000178  spi_sdo_hi
00017E  spi_sdo_lo
000184  spi_sck_hi
00018A  spi_sck_lo
0001C4  spi_cs_hi
000174  spi_cs_lo
000190  spi_rw
00016E  FT800_PD_hi
000140  FT800_PD_lo
000228  FT800memWrite8
000262  FT800memWrite16
0002A8  FT800memWrite32
00084C  FT800memWriteStr
0001C8  FT800_HostCmdWrite
0001DC  FT800memRead8
000640  FT800memRead16
000C64  FT800memRead32
0006A6  Start_CMDOffset
0006EC  incCMDOffset
0008C2  End_incCMDOffset
000BCA  Touch_Calibrate
000004  @const290
000808  @SPRINTF
000824  @PSTRINGC_292
000710  Start_CMDList
000B18  End_CMDList
000900  Text_CMD
000318  FT800_Initial
000D7E  Conv_hex_to_Ascii
000D3C  @DIV1616
001684  Update_Screen
000018  @const299
000038  @const300
00004E  @const301
000068  @const302
00008A  @const304
0000AC  @const306
0000CE  @const308
0000F0  @const310
000112  @const312
001D30  User_App
001F70  @cinit


User Memory space: 

User Memory space: 

Project Directory:
    C:\Users\yooyod\Documents\ETT_Work\VM800C_FT800\ETT_Example\PIC_18F8722\Ex3_TFT43_RegTouch\3_1_RdReg_Touch\

Project Files:
    Ex3_1_TFT43_RdReg_Touch.c                               [23-ÁÕ.¤.-14 14:20  CRC=7DE64499]
    ..\..\..\..\..\..\..\..\..\Program Files\PICC\devices\18F8722.h [27-¡.¤.-11 18:03  CRC=67760F74]
    ..\..\..\..\..\..\..\..\..\Program Files\PICC\drivers\stdio.h [31-¡.¤.-07 13:24  CRC=4E4534F4]
    ..\..\..\..\..\..\..\..\..\Program Files\PICC\drivers\string.h [14-¡.¤.-11 10:13  CRC=23EDEC8F]
    ..\..\..\..\..\..\..\..\..\Program Files\PICC\drivers\stddef.h [16-¡.¤.-10 09:27  CRC=897CEC6C]
    ..\..\..\..\..\..\..\..\..\Program Files\PICC\drivers\ctype.h [03-Á.¤.-08 13:55  CRC=2D1F019F]

Source signature=3B4A653A

Units:
    C:\Users\yooyod\Documents\ETT_Work\VM800C_FT800\ETT_Example\PIC_18F8722\Ex3_TFT43_RegTouch\3_1_RdReg_Touch\Ex3_1_TFT43_RdReg_Touch (main)

Compiler Settings:
    Processor:      PIC18F8722
    Pointer Size:   16
    ADC Range:      0-255
    Opt Level:      9
    Short,Int,Long: UNSIGNED: 1,8,16
    Float,Double:   32,32

Output Files:
    Errors:      Ex3_1_TFT43_RdReg_Touch.err
    Ext Symbols: Ex3_1_TFT43_RdReg_Touch.esym
    INHX32:      Ex3_1_TFT43_RdReg_Touch.hex
    Symbols:     Ex3_1_TFT43_RdReg_Touch.sym
    List:        Ex3_1_TFT43_RdReg_Touch.lst
    Debug/COFF:  Ex3_1_TFT43_RdReg_Touch.cof
    Project:     Ex3_1_TFT43_RdReg_Touch.PJT
    Call Tree:   Ex3_1_TFT43_RdReg_Touch.tre
    Statistics:  Ex3_1_TFT43_RdReg_Touch.STA
