000     @SCRATCH
001     @SCRATCH
001     _RETURN_
002     @SCRATCH
003     @SCRATCH
004-005 strtok.save
006-007 DL_Offset
008-009 cmdOffset
00A-00B cmdBufferRd
00C-00D cmdBufferWr
00E     ft800Gpio
00F     num_cha
010-011 tc_x
012-013 tc_y
014     tb1
015     tb2
016     tb3
017     tb4
018     tb5
019     fag
01A     sigA
01B     sigB
01C     sigC
01D     sigD
01E     sigE
01F     sigF
020-021 intA
022-023 intB
024-025 intC
026-027 intD
028-029 intE
02A-02B intF
02C-02D fracA
02E-02F fracB
030-031 fracC
032-033 fracD
034-035 fracE
036-037 fracF
038-039 @sprintf_string
03A     FT800_HostCmdWrite.Command
03A-03D FT800memRead8.addr
03A-06B User_App.strbuf
03A-03D Initial_Calibrate.val
03A     FT800_Initial.@SCRATCH1
03B     FT800_Initial.@SCRATCH2
03C     FT800_Initial.@SCRATCH3
03D     FT800_Initial.@SCRATCH4
03E     FT800memRead8.data8
03E     Initial_Calibrate.@SCRATCH1
03F     FT800memRead8.@SCRATCH1
03F     Initial_Calibrate.@SCRATCH2
040     FT800memRead8.@SCRATCH2
040     Initial_Calibrate.@SCRATCH3
041     FT800memRead8.@SCRATCH3
041     Initial_Calibrate.@SCRATCH4
042     FT800memRead8.@SCRATCH4
042     Initial_Calibrate.@SCRATCH5
043     FT800memRead8.@SCRATCH5
06C-09D Update_Screen.strbuf
06C-06F Touch_Read_XY.xy
06C-06D Touch_Detect.td
06C     ThaiLand_Song.vol
06C     User_App.@SCRATCH1
06D     Sound_Effect.vol
06D     ThaiLand_Song.@SCRATCH1
06E     @delay_ms1.P1
06E-06F Sound_Effect.midi
070-073 FT800memRead32.addr
070-071 Sound_Effect.effect
070     Touch_Read_XY.@SCRATCH1
071     Touch_Read_XY.@SCRATCH2
072-075 FT800memWrite8.addr
072     Touch_Read_XY.@SCRATCH3
072     Sound_Effect.@SCRATCH1
073     Touch_Read_XY.@SCRATCH4
073     Sound_Effect.@SCRATCH2
074-077 FT800memRead32.data32
074     Touch_Read_XY.@SCRATCH5
076     FT800memWrite8.data8
077     FT800memWrite8.@SCRATCH1
078-07B FT800memRead32.dat
078     FT800memWrite8.@SCRATCH2
079     FT800memWrite8.@SCRATCH3
07A     FT800memWrite8.@SCRATCH4
07B     FT800memWrite8.@SCRATCH5
07C     FT800memRead32.@SCRATCH1
07D     FT800memRead32.@SCRATCH2
07E     FT800memRead32.@SCRATCH3
07F     FT800memRead32.@SCRATCH4
080     FT800memRead32.@SCRATCH5
09E-0A1 Start_CMDList.screen_color
09E-09F Text_CMD.str
09E-0A1 EdgeStripL_DL.x1
09E-0A1 Rect_DL.x1
09E     End_CMDList.@SCRATCH1
09E     @PSTRINGC_301.@SCRATCH1
09F     End_CMDList.@SCRATCH2
09F     @PSTRINGC_301.@SCRATCH2
0A0-0A1 Text_CMD.x
0A0     End_CMDList.@SCRATCH3
0A0     @PSTRINGC_301.@SCRATCH3
0A1     @SPRINTF.P1
0A1     End_CMDList.@SCRATCH4
0A2-0A5 FT800memRead16.addr
0A2-0A5 Rect_DL.y1
0A2-0A3 Text_CMD.y
0A2-0A5 EdgeStripL_DL.y1
0A2     Start_CMDList.@SCRATCH1
0A3     Start_CMDList.@SCRATCH2
0A4-0A5 Text_CMD.font
0A4     Start_CMDList.@SCRATCH3
0A5     Start_CMDList.@SCRATCH4
0A6-0A7 FT800memRead16.data16
0A6-0A9 Rect_DL.x2
0A6-0A9 EdgeStripL_DL.x2
0A6-0A7 Text_CMD.opt
0A6     Start_CMDList.@SCRATCH5
0A7     Start_CMDList.@SCRATCH6
0A8-0A9 FT800memRead16.dat
0A8-0AB Text_CMD.tx_color
0A8     Start_CMDList.@SCRATCH7
0A9     Start_CMDList.@SCRATCH8
0AA-0AD Rect_DL.y2
0AA-0AD EdgeStripL_DL.y2
0AA     FT800memRead16.@SCRATCH1
0AB     FT800memRead16.@SCRATCH2
0AC-0AD End_incCMDOffset.currentOffset
0AC     FT800memRead16.@SCRATCH3
0AC     Text_CMD.@SCRATCH1
0AD     FT800memRead16.@SCRATCH4
0AD     Text_CMD.@SCRATCH2
0AE     End_incCMDOffset.commandSize
0AE-0B1 EdgeStripL_DL.x3
0AE-0AF Rect_DL.wd
0AE     FT800memRead16.@SCRATCH5
0AE     Text_CMD.@SCRATCH3
0AF-0B0 End_incCMDOffset.newOffset
0AF     Text_CMD.@SCRATCH4
0B0-0B3 Rect_DL.rect_color
0B0-0B3 FT800memWriteStr.addr
0B0-0B3 FT800memWrite16.addr
0B0     Text_CMD.@SCRATCH5
0B1     End_incCMDOffset.@SCRATCH1
0B1     Text_CMD.@SCRATCH6
0B2-0B5 EdgeStripL_DL.y3
0B2     End_incCMDOffset.@SCRATCH2
0B2     Text_CMD.@SCRATCH7
0B3     Text_CMD.@SCRATCH8
0B4-0B5 FT800memWrite16.data16
0B4-0B7 Rect_DL.xy1
0B4-0B5 FT800memWriteStr.str
0B6-0B7 EdgeStripL_DL.wd
0B6-0B7 FT800memWriteStr.i
0B6     FT800memWrite16.@SCRATCH1
0B7     FT800memWrite16.@SCRATCH2
0B8-0BB Rect_DL.xy2
0B8-0BB EdgeStripL_DL.line_color
0B8     FT800memWrite16.@SCRATCH3
0B8     FT800memWriteStr.@SCRATCH1
0B9     FT800memWrite16.@SCRATCH4
0B9     FT800memWriteStr.@SCRATCH2
0BA     FT800memWrite16.@SCRATCH5
0BA     FT800memWriteStr.@SCRATCH3
0BB     FT800memWriteStr.@SCRATCH4
0BC-0BF EdgeStripL_DL.xy1
0BC     FT800memWriteStr.@SCRATCH5
0BC     Rect_DL.@SCRATCH1
0BD     Rect_DL.@SCRATCH2
0BE     Rect_DL.@SCRATCH3
0BF     Rect_DL.@SCRATCH4
0C0-0C3 EdgeStripL_DL.xy2
0C0     Rect_DL.@SCRATCH5
0C1     Rect_DL.@SCRATCH6
0C2     Rect_DL.@SCRATCH7
0C3     Rect_DL.@SCRATCH8
0C4-0C7 EdgeStripL_DL.xy3
0C8-0C9 incCMDOffset.currentOffset
0C8     EdgeStripL_DL.@SCRATCH1
0C9     EdgeStripL_DL.@SCRATCH2
0CA     incCMDOffset.commandSize
0CA     EdgeStripL_DL.@SCRATCH3
0CB-0CC incCMDOffset.newOffset
0CB     EdgeStripL_DL.@SCRATCH4
0CC     EdgeStripL_DL.@SCRATCH5
0CD     EdgeStripL_DL.@SCRATCH6
0CE     EdgeStripL_DL.@SCRATCH7
0CF     EdgeStripL_DL.@SCRATCH8
0D0-0D3 FT800memWrite32.addr
0D4-0D7 FT800memWrite32.data32
0D8     FT800memWrite32.@SCRATCH1
0D9     FT800memWrite32.@SCRATCH2
0DA     FT800memWrite32.@SCRATCH3
0DB     FT800memWrite32.@SCRATCH4
0DC     FT800memWrite32.@SCRATCH5
0DD     spi_rw.Db
0DE     spi_rw.bt
0DF     spi_rw.result
0E0     spi_rw.@SCRATCH1
F71     CCP_5
F71     CCP_5_LOW
F72     CCP_5_HIGH
F74     CCP_4_LOW
F74     CCP_4
F75     CCP_4_HIGH
F83     PSP_DATA
FB4.6   C1OUT
FB4.7   C2OUT
FB8     CCP_3
FB8     CCP_3_LOW
FB9     CCP_3_HIGH
FBB     CCP_2_LOW
FBB     CCP_2
FBC     CCP_2_HIGH
FBE     CCP_1_LOW
FBE     CCP_1
FBF     CCP_1_HIGH
FE1-FE2 @READ_PACKED_MEMORY.P1
FE1-FE2 @WRITE_PACKED_MEMORY.P2
FE9-FEA @READ_PACKED_MEMORY.P1
FE9-FEA @WRITE_PACKED_MEMORY.P2
FE9-FEA @WRITE_PROGRAM_MEMORY.P3
FE9-FEA @READ_PROGRAM_MEMORY.P4
FF6-FF8 @WRITE_PROGRAM_MEMORY.P1
FF6-FF8 @READ_PROGRAM_MEMORY.P2

ROM Allocation:
00005A  @delay_ms1
002D4E  MAIN
000048  init_port
00008C  spi_sdo_hi
000092  spi_sdo_lo
000098  spi_sck_hi
00009E  spi_sck_lo
0000D8  spi_cs_hi
000088  spi_cs_lo
0000A4  spi_rw
000082  FT800_PD_hi
000054  FT800_PD_lo
00013C  FT800memWrite8
000176  FT800memWrite16
0001BC  FT800memWrite32
000960  FT800memWriteStr
0000DC  FT800_HostCmdWrite
0000F0  FT800memRead8
000750  FT800memRead16
002024  FT800memRead32
0007B6  Start_CMDOffset
0007FE  incCMDOffset
0009E4  End_incCMDOffset
001FF0  Touch_Detect
0020FE  Touch_Read_XY
000554  Initial_Calibrate
001170  Sound_Effect
0011CA  ThaiLand_Song
000822  Start_CMDList
0010BA  End_CMDList
000A22  Text_CMD
002136  Rect_DL
000C42  EdgeStripL_DL
00022C  FT800_Initial
0024B6  Update_Screen
000004  @const299
00091A  @SPRINTF
000938  @PSTRINGC_301
0027D6  User_App
000020  @const305
000034  @const306
002D4E  @cinit


User Memory space: 

User Memory space: 

Project Directory:
    C:\Users\yooyod\Documents\ETT_Work\VM800C_FT800\ETT_Example\PIC_18F8722\Ex3_TFT43_RegTouch\3_2_WrReg_Touch\

Project Files:
    Ex3_2_TFT43_WrReg_Touch.c                               [23-ÁÕ.¤.-14 14:36  CRC=116FBC26]
    ..\..\..\..\..\..\..\..\..\Program Files\PICC\devices\18F8722.h [27-¡.¤.-11 18:03  CRC=67760F74]
    ..\..\..\..\..\..\..\..\..\Program Files\PICC\drivers\stdio.h [31-¡.¤.-07 13:24  CRC=4E4534F4]
    ..\..\..\..\..\..\..\..\..\Program Files\PICC\drivers\string.h [14-¡.¤.-11 10:13  CRC=23EDEC8F]
    ..\..\..\..\..\..\..\..\..\Program Files\PICC\drivers\stddef.h [16-¡.¤.-10 09:27  CRC=897CEC6C]
    ..\..\..\..\..\..\..\..\..\Program Files\PICC\drivers\ctype.h [03-Á.¤.-08 13:55  CRC=2D1F019F]

Source signature=CED3DCC7

Units:
    C:\Users\yooyod\Documents\ETT_Work\VM800C_FT800\ETT_Example\PIC_18F8722\Ex3_TFT43_RegTouch\3_2_WrReg_Touch\Ex3_2_TFT43_WrReg_Touch (main)

Compiler Settings:
    Processor:      PIC18F8722
    Pointer Size:   16
    ADC Range:      0-255
    Opt Level:      9
    Short,Int,Long: UNSIGNED: 1,8,16
    Float,Double:   32,32

Output Files:
    Errors:      Ex3_2_TFT43_WrReg_Touch.err
    Ext Symbols: Ex3_2_TFT43_WrReg_Touch.esym
    INHX32:      Ex3_2_TFT43_WrReg_Touch.hex
    Symbols:     Ex3_2_TFT43_WrReg_Touch.sym
    List:        Ex3_2_TFT43_WrReg_Touch.lst
    Debug/COFF:  Ex3_2_TFT43_WrReg_Touch.cof
    Project:     Ex3_2_TFT43_WrReg_Touch.PJT
    Call Tree:   Ex3_2_TFT43_WrReg_Touch.tre
    Statistics:  Ex3_2_TFT43_WrReg_Touch.STA
