───────────────────────────────────────
Parallax Propeller Chip Project Archive
───────────────────────────────────────

 Project :  "SimplePropellerAssemblyDebugger_ReadMeDemo"

Archived :  Wednesday, December 19, 2007 at 10:48:38 AM

    Tool :  Propeller Tool version 1.05.8


            SimplePropellerAssemblyDebugger_ReadMeDemo.spin
              │
              └──SimplePropellerAssemblyDebugger.spin
                   │
                   └──FullDuplexSerialPlus_Plus.spin





Simple Propeller Assembly Debugger (SPAD)  
 

  At last, a debugging tool that works exactly like the Basic Stamp. Yes,
 the old reliable Stamp commands debugChar, debugStr, debugDec, debugBin,
 debugInChar, debugInDec, debugWatchDog and debugDelay may be inserted directly 
into your propeller assembly code to provide output to and input from your PC just 
as you did with Stamp debug commands.
 Writing and learning assembly language code is very easy when you can control your 
output/input to your PC directly from your assembly code. Now you can stop your assembly code at 
any point using a simple debugInChar command. Your assembly routine can printout characters and 
strings directly to your PC and input data directly from your PC keyboard. A 32-bit multiply and 
divide routines are also provided .
 


────────────────────
Parallax, Inc.
www.parallax.com
support@parallax.com
USA 916.624.8333