───────────────────────────────────────
Parallax Propeller Chip Project Archive
───────────────────────────────────────

 Project :  "VGA_HiRes_Text_Demo"

Archived :  Monday, April 30, 2007 at 4:30:00 PM

    Tool :  Propeller Tool version 1.05.6


            VGA_HiRes_Text_Demo.spin
              │
              ├──VGA_HiRes_Text.spin
              │
              └──Mouse.spin






This object generates a 1024x768 VGA signal which contains 128 columns x 64 rows of 8x12 characters.
Each row can have a unique forground/background color combination and each character can be inversed. 
There are also two cursors which can be independently controlled (ie. mouse and keyboard). 
A sync indicator signals each time the screen is refreshed (you may ignore).


────────────────────
Parallax, Inc.
www.parallax.com
support@parallax.com
USA 916.624.8333