DESCRIPTION


This ATMEL ISP software allows to program all our FLASH
C51 parts. 

This software is named FLIP, which stands  for FLexible
In-system Programmer.


DOWNLOAD


This program can be downloaded from our website:
http://www.atmel.com


MAIN FEATURES

- performs In-System Programming  through RS232, USB or 
  CAN interfaces.

- may  be used  through its  intuitive  Graphical  User
  Interface  or launched  from a DOS  window  (see  the
  batchisp manual), from an  embedded software IDE like
  KEIL's uVision2,  or even from  your own  application
  (see the ISP Functions Library manual).

- runs under Windows 9x / Me / NT / 2000 / XP.

- supports  Intel  MCS-86 Hexadecimal  Object,  Code 88
  file format for data file loading and saving.

- buffer  editing  capabilities :  fill,  search,  copy,
  reset, modify, goto.

- target  device  memory control :  erase,  blank check,
  program,  verify,  read,  security level  and special
  bytes reading and setting.

- parts serialization capability (from batchisp only).

- AutoISP  allows ISP  hardware conditions to be set by
  software.

- the demo  mode emulates ISP  operations  without  any
  target hardware.

- the debug  mode lets  you  log  the  traffic  on  the
  selected medium.

- on-line help.


KNOWN BUGS AND LIMITATIONS


See the Changes file for information about  the current
version.

PROBLEMS


If you find any problem, please report it to the Atmel's
hotline.

e-mail address: mcu@atmel.com


